|  |  |  |  |
| --- | --- | --- | --- |
| BOILING POINT (INITIAL): | 147-159°C | SPECIFIC GRAVITY: | 0.8 typical at 25°C |
| SOLUBILITY IN WATER: | Immiscible | pH: | Not applicable |
| VAPOR PRESSURE: | Not determined | VAPOR DENSITY: | Not determined |
| PERCENT VOLATILE: | Not determined | VOC: | Not determined |
| COEFFICIENT OF WATER/OIL DISTRIBUTION: | Not determined | APPEARANCE/ODOR: | Cloudy white liquid spray with strong solvent odor |
| FLASHPOINT: | 33°C | FLAMMABLE LIMITS: | LEL 0.7% UEL 6.0% |



**TECHNICAL DATA SHEET**

WD-40 Specialist®

DRY PTFE

|  |  |  |
| --- | --- | --- |
| **Product Description** | | **PACKAGING** |
| WD-40 Specialist Dry PTFE provides enhanced lubrication without an oily residue. Best used where cleanliness and maximum performance are required as it dries leaving behind a clear dry lubricating film that resists dirt, dust and oil buildups. Great for reducing friction and wear on blades and bits, door and window tracks, slides, conveyor belts, rollers, hinges, table saws, lathes, power tools and equipment. Keeps your equipment running smoothly with long-lasting corrosion protection. | |  |
| **Applications** | **Features & Benefits** |
| * Blades & Bits * Door & Window Tracks * Slides * Rollers * Hinges * Conveyor Belts * Power Tools & Equipment | * Lubricates Blades & Bits * Won't Attract Dirt & Dust * Great for Table Saws, Drills & Lathes * Safe on Wood, Glass, Metal, and Most Plastics\* * Temperature Ranges from -50°F to 500°F   \* Always test on an inconspicuous area before use |
| **fluid Properties** | | |

|  |
| --- |
| **Packaging Specifications** |
| |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **SKU Codes and Description** | | | **Individual Item (Consumer Unit)** | | | | | **Carton (Traded Unit)** | | | | | | **Pallet Information** | | | | | | **Case Codes** | **Unit Codes** | **Product Description** | **Dimensions (mm)** | | | **Cubic Volume (cm³)** | **Gross Weight (kg)** | **Dimensions (mm)** | | | **Cubic Volume (cm³)** | **Gross Weight (kg)** | **Units**  **Per**  **Carton** | **Consumer Units Per Pallet** | **Dimensions (mm)** | | | **Gross Weight (kg)** | | **Width** | **Depth** | **Height** | **Width** | **Depth** | **Height** | **Width** | **Depth** | **Height** | | 21105 | 21005 | WD-40 Specialist Anti Friction Dry PTFE Lubricant 150g Smart Straw | 53 | 53 | 179 | 503 | 0.23 | 118 | 165 | 191 | 3719 | 1.455 | 6 | 1830 | 1165 | 1165 | 1105 | 477.78 | |
|  |
| **Directions** |
| Shake can well. Flip straw up for narrow spray or down for wide spray. Spray directly on surface to be lubricated.    **TECHNICAL DATA SHEET**  WD-40 Specialist®  DRY PTFE |
| **hazard identification** |
| HAZARDOUS SUBSTANCE. DANGEROUS GOODS. According to the WHS Regulations and the ADG Code.  **DANGER! Extremely flammable aerosol. Pressurized container: may burst if heated. May cause an allergic skin reaction. May cause drowsiness or dizziness. May be fatal if swallowed and enters airways. Harmful to aquatic life with long lasting effects. Repeated exposure may cause skin dryness or cracking.** Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking. Do not spray on an open flame or other ignition source. Do not pierce or burn, even after use. Avoid breathing mist or vapors. Use only outdoors or in a well-ventilated area. Contaminated work clothing should not be allowed out of the workplace. Avoid release to the environment. Wear protective gloves. If swallowed: Immediately call a POISON CENTER or doctor. DO NOT induce vomiting. If on skin: Wasg with plenty of soap and water. Take off contaminated clothing and wash it before reuse. If inhaled: Remove person to fresh air and keep comfortable for breathing. If discomfort persists, see a doctor. Additional information is listed in the safety data sheet. |
| **Storage** |
| Store in a cool, dry, ventilated area away from incompatible materials. Protect from physical damage. Do not store in direct sunlight, near open flames or above temperatures greater than 50°C. |
| **Regulatory Information** |
| **Montreal Protocol (Ozone Depleting Substances):** None present. **The Stockholm Convention (Persistent Organic Pollutants):** None present. **The Rotterdam Convention (Prior Informed Consent):** Not applicable. **Basel Convention:** Not applicable. **International Convention for the Prevention of Pollution from Ships (MARPOL):** Not applicable. **Standard for the Uniform Scheduling of Medicines and Poisons (SUSMP):** Not applicable  **Australian Inventory of Chemical Substances:** All the components of this product are listed on the AICS inventory  **New Zealand Inventory:** All the ingredients comply with the HSNO regulations |

Level 2, 41 Rawson Street, Epping, NSW 2121 Australia  **Version: 1.0**

**wd40.com.au**